==========================================================================
                DICE2 Project for DICE-Kit Evaluation Board 
==========================================================================
                   Fujitsu Microelectronics Europe GmbH                       
                 http://emea.fujitsu.com/microelectronics 
                                                            
 The following  software  is for  demonstration  purposes only.  It is not
 fully  tested, nor validated  in order  to fullfill  its task  under  all
 circumstances.  Therefore,  this software or  any part of it must only be
 used in an evaluation laboratory environment.                        
 This software is subject to the rules of our standard DISCLAIMER, that is
 delivered with our  SW-tools on the Fujitsu Microcontrollers CD 
 (V3.4 or higher "\START.HTM") or on our Internet Pages:
 http://www.fme.gsdc.de/gsdc.htm
 http://emea.fujitsu.com/microelectronics 
==========================================================================
               
History
Date      Ver     Author  Softune     Description
16.09.05  1.0     HWE     V30L32      original version for MB90F357
04.01.07  3.0     HWE     V30L33R09   new headerfiles supporting MB90350/5
==========================================================================

This is Demoproject for the DICE-Kit Evaluation-Board. 
It includes some basic settings for e.g. Linker, C-Compiler 
which must be checked and modified in detail, 
corresponding to the user application.

Description:
This projects simulates two dices.
SEG1 is dice1 and can be started by pressing key SW2 (INT8)
SEG2 is dice2 and can be started by pressing key SW3 (INT9)
After a while the started dice will stop displaying a value from 1..6.

Note:
Remove jumper JP2 (External watchdog is not supported by this project)